{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":28,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":10,"rows_kept":20,"merged":[[0,0,0,9],[19,1,19,7]],"flags":["formulas_cached_only"]}
["中国—马来西亚钦州产业园区启动区综合配套建设项目一期项目地下停车场地坪漆项目清单文件"]
["序号","名称","简图","规格(cm)","材质","单位","数量","单价(元)","金额","（备注)"]
[1,"橡塑警示护角",null,"长78-80×宽18-20×厚5.0-6.0的橡塑警示护角，国标以上标准","橡塑","个",1190,null,null,"包工包料包安装含税"]
[2,"流线型减速路拱",null,"长50×宽30×厚3.5，国标以上标准","橡胶","m",120,null,null,"包工包料包安装含税"]
[3,"橡塑车轮定位器",null,"规格：53*14*8cm；置于停车位后线距前1.1米处，采用10*120拉爆螺丝安装牢固，可有效的防止车辆在进入车位时碰撞车后物体或墙壁，国标以上标准","橡塑","个",1064,null,null,"包工包料包安装含税"]
[4,"车库导向牌",null,"60cm*120cm,80cm*120cm,80cm*140cm,80cm*160cm,100cm*600cm.采用是进口美国3M工程反光膜，电脑割字、机械贴膜、反光效果好、耐用性强、在自然环境中可保持七年内不褪色，不脱落、不断裂等。吊牌采用扁通悬挂，设置位要整齐规范，风格一致,位置适当，视线良好，符合GB2894-88《安全标志》的规定，国标以上标准","铝合金镀锌板","㎡",216.9,null,null,"包工包料包安装含税"]
[5,"广角镜",null,"60cm（直径）/国标，国标以上标准","国标","个",4,null,null,"包工包料包安装含税"]
[6,"非机动车库地面导向箭头",null,"7cm（导向箭头宽）/70cm（导向箭头长）","特种标线漆","个",53,null,null,"包工包料包安装含税"]
[7,"地面导向箭头",null,"15cm（导向箭头宽）/300cm（导向箭头长）","特种标线漆","个",181,null,null,"包工包料包安装含税"]
[8,"实/虚直线",null,"15cm/宽","特种标线漆","m",5283.79,null,null,"包工包料包安装含税"]
[9,"车位编号",null,"字高30cm模版字","特种标线漆","个",531,null,null,"包工包料包安装含税"]
[10,"车位线",null,"530cm（车位长)×240cm（车位宽)×15cm（线宽）","特种标线漆","㎡",1269.03,null,null,"包工包料包安装含税"]
[11,"环氧地坪漆（停车位区域，施工厚度2mm）",null,"1、基层打磨：打磨整体地面（为增加附着力），铲除原有开裂、空鼓地面（预防起皮、脱层现象），清扫、除尘，要求地面较平整、干净、干燥\n2、裂缝、坑洼处理：用树脂+石英砂填补，去除浮浆，要求较平整、干净\n3、底漆层：整体刮涂东升固化剂+DS-10＃无溶剂环氧底漆（封闭地坪表面尘土，使底漆渗透地面，增加与地面的附着力）\n4、中涂层：整体刮涂东升DS-410无溶剂环氧中涂（增加地坪强度)，根据设计施工厚度增减施工遍数。                                            5、面漆层：整体滚涂东升DS-146无溶剂环氧面漆，颜色均匀一致。 养护7天（养护期间不得使用；不得用水和任何溶剂冲洗地面、锐器磨擦等）","环氧地坪漆（2mm,光面）","㎡（中灰色、绿色、淡铁蓝）",11366.04,null,null,"包工包料包安装含税"]
[12,"\n环氧地坪漆（行车通道区，施工厚度3mm）",null,"1、基层打磨：打磨整体地面（为增加附着力），铲除原有开裂、空鼓地面（预防起皮、脱层现象），清扫、除尘，要求地面较平整、干净、干燥\n2、裂缝、坑洼处理：用树脂+石英砂填补，去除浮浆，要求较平整、干净\n3、底漆层：整体刮涂东升固化剂+DS-10＃无溶剂环氧底漆（封闭地坪表面尘土，使底漆渗透地面，增加与地面的附着力）\n4、中涂+石英砂层：整体刮涂东升DS-410无溶剂环氧中涂+石英砂（增加地坪强度、耐磨度）。待完全干透进行整体细磨，根据设计施工厚度增减施工遍数。                                            5、中涂层：整体刮涂DS-410无溶剂环氧中涂，增加平整度及地坪强度                                      6、面漆层：整体滚涂东升DS-146无溶剂环氧面漆，颜色均匀一致。 \n养护7天（养护期间不得使用；不得用水和任何溶剂冲洗地面、锐器磨擦等）","环氧地坪漆（3mm,光面）","㎡，（中灰色、绿色、淡铁蓝）",8116.5,null,null,"包工包料包安装含税"]
[13,"环氧地坪漆（防滑坡道，粗面，施工厚度5mm）",null,"1、基层打磨：打磨整体地面（为增加附着力），铲除原有开裂、空鼓地面（预防起皮、脱层现象），清扫、除尘，要求地面较平整、干净、干燥\n2、裂缝、坑洼处理：用树脂+石英砂填补，去除浮浆，要求较平整、干净\n3、底漆层：整体刮涂东升固化剂+DS-10＃无溶剂环氧底漆（封闭地坪表面尘土，使底漆渗透地面，增加与地面的附着力）\n4、中涂层：整体滚涂东升DS-410无溶剂环氧中涂（增加地坪强度)，均匀挥洒东升专用彩砂，穿钉鞋用扫把将表面扫平整，待完全干透再次清扫浮沙，根据设计施工厚度增减施工遍数。                                                             5、面漆层：整体滚涂东升DS-146无溶剂环氧面漆+罩光漆，颜色均匀一致。 养护7天（养护期间不得使用；不得用水和任何溶剂冲洗地面、锐器磨擦等）","环氧地坪漆（5mm,粗面）","㎡，（中灰色、绿色、淡铁蓝）",867.88,null,null,"包工包料包安装含税"]
[14,"墙体美化",null,"室内美化墙漆","环氧墙漆","㎡，（根据地面颜色确定）",4277.68,null,null,"包工包料包安装含税"]
[15,"踢脚线",null,"15cm高弹踢脚线","高弹乳胶漆，底漆，面漆","m，（根据地面颜色确定）",3827.46,null,null,"包工包料包安装含税"]
[16,"墙面及柱子区域标识",null,"字高60cm模版字","环保水性标线漆","个",985,null,null,"包工包料包安装含税"]
[17,"反光道钉及反光轮廓标",null,"钻石级反光膜达到部颁所规定标准；由高强度塑料，双面反光；耐紫外光，抗老化，耐盐碱腐蚀，耐风沙磨损；作用：反光导体，指引车辆正常行驶；有效地减少驾驶员因视觉差度。（一般每1米一个）","反光道钉及反光轮廓标","个",300,null,null,"包工包料包安装含税"]
[18,"合计造价金额",{"$nulls":7},"包工包料包安装含税"]