{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["施工招标工程量清单"],"not_rendered":{"external_links":12,"defined_names":123},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"施工招标工程量清单","index":0,"n_rows":110,"n_cols":5,"rows_kept":110,"merged":[[0,0,0,4],[1,0,1,4]],"flags":["formulas_cached_only"]}
["施工工程量清单"]
["工程名称：中马钦州产业园区友谊大道中段工程项目部临时生活用电项目"]
["序号","项 目 名 称 及 规 范","单 位","数 量","备注"]
[1,"基础建设工程量"]
[1.1,"土（石）方工程"]
["1.1.1","挖沟槽土方"]
[null,"机械挖土方、三类土  深1.5m以内","m³",11.33]
["1.1.2","回填土"]
[null,"夯实、场地平整 回填土  夯填","m³",4.73]
["1.1.3","余土弃置"]
[null,"运距1km","m³",{"v":6.6,"d":"6.60"}]
[1.2,"砌筑工程"]
["1.2.1","石基础"]
[null,"MU10毛石 条形 M7.5水泥砂浆砌筑","m³",5.66]
["1.2.2","实心砖墙"]
[null,"多孔砖  240mm  外墙  M7.5混合砂浆","m³",6.97]
["1.2.3","零星砌筑"]
[null,"电缆沟 多孔砖 M7.5水泥砂浆","m³",0.27]
[1.3,"混凝土钢筋混凝土工程"]
["1.3.1","垫层"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C15","m³",1.94]
["1.3.2","基础梁"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C25","m³",0.85]
["1.3.3","构造柱"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C25","m³",0.65]
["1.3.4","过梁"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C25","m³",0.09]
["1.3.5","有梁板"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C25","m³",1.43]
["1.3.6","雨棚"]
[null,"1.混凝土种类:商品砼2.混凝土强度等级:C25","m³",1.35]
["1.3.7","现浇构件钢筋"]
[null,"10以内螺纹圆钢","t",0.066]
[null,"10以上螺纹圆钢","t",0.019]
["1.3.8","屋面刚性防水层钢筋网片"]
[null,"内配4@100双向钢筋网与屋面板预埋10钢筋头绑牢","㎡",8.64]
[1.4,"屋面及防水工程"]
["1.4.1","屋面防水卷材"]
[null,"4厚SBS改性沥青防水卷材防水层","㎡",34.56]
["1.4.2","屋面水泥砂浆找平层"]
[null,"20厚1:2.5水泥砂浆找平层","㎡",8.64]
["1.4.3","雨棚砂浆防水"]
[null,"水泥砂浆掺5%防水剂抹面压光","㎡",1.08]
[1.5,"楼地面工程"]
["1.5.1","细石混凝土楼地面"]
[null,"面层厚度、混凝土强度等级:30厚C20细石混凝土","㎡",6.14]
["1.5.2","零星项目砂浆找平"]
[null,"1.基层类型、部位:电缆沟2.底层厚度、砂浆种类、配合比:15厚1:3水泥砂浆3.面层厚度、砂浆种类、配合比:5厚1:2.5水泥砂浆","㎡",3.84]
[1.6,"墙、柱面工程"]
["1.6.1","外墙面一般抹灰"]
[null,"10厚聚合物防水砂浆找平层","㎡",28.24]
["1.6.2","内墙面一般抹灰"]
[null,"1、5厚1:0.3:3水泥石灰膏砂浆；2、12厚1:1:6水泥石灰膏砂浆打底；3、刷界面剂一道(素水泥浆一道)","㎡","25.55"]
["1.6.3","电缆沟水泥砂浆找平层"]
[null,"20厚1：2.5水泥砂浆","㎡","4.68"]
[1.7,"天棚工程"]
["1.7.1","天棚抹灰","㎡","4.68"]
[1.8,"门窗工程"]
["1.8.1","金属门"]
[null,"钢制乙级防火门","㎡","2.64"]
[1.8,"措施费","项","1"]
[2,"安装工程"]
[2.1,"电气设备安装工程"]
["2.2.2","油浸电力变压器"]
[null,"1.型号:S11-M-250kVA 2、2.安装部位:配电屋顶","台","1"]
["2.2.3","电力电缆"]
[null,"1.名称:高压电缆；2.规格:YJV22-8.7/15kV-3*95mm23；敷设方式、部位:室外管道敷设原配电房至新建配电室；4.电压等级(kV):10kV","m","600.00"]
["2.2.4","低压电容器柜"]
[null,"1.电容补偿箱；2.型号：4*20+2*10kvar TDS-13SZ-20(10)","台","1"]
["2.2.4","配电柜"]
[null,"1.低压出线配电箱；2、2.塑壳断路器 400H/3310","台","1"]
[null,"1、计量柜；2、规格600A","台","1"]
["2.2.5","10kV避雷器"]
[null,"型号:YH5WS-17/50","组","1"]
["2.2.6","高压熔断器"]
[null,"1.名称：10kV跌落式熔断器；2.型号:12kV/200-25A","组","1"]
["2.2.7","导线、进户线架设"]
[null,"1.名称：10kV铝芯交联聚乙烯绝缘架空电缆；2.型号:JKLYJ-95mm2","米","30"]
["2.2.8","电杆组立"]
[null,"1.名称:12m高强度部分预应力锥形杆；2.规格：BY-Z-190×12-68kN.m；3.杆号：N1；4、三牌","根","1"]
["2.2.9","横担组装"]
[null,"1.名称:瓷横担绝缘子；2.型号:SC-210","组","6"]
[null,"1.名称:跌落式熔断开关横担；2.型号:L75×8×1600","组","1"]
[null,"1.名称:避雷器横担；2.型号:L63×6×1600","组","1"]
[null,"1.名称:单杆引线担；2.型号:L63×8×1600","组","2"]
[2.3,"措施费","项",1]
[3,"辅助性材料安装"]
["3.3.1","焊、压接线端子"]
[null,"型号:DT-95mm2","个","6"]
[null,"型号:DTL-95mm2","个","12"]
[null,".型号:DTL-240mm2","个","16"]
[null,".型号:DT-70mm2","个","8"]
["3.3.2","配线"]
[null,"1.名称:黄绿双色线；2.型号:BLVV-50mm2","米","110"]
[null,"名称:10kV三相短路接地线","组","1"]
["3.3.3","接地"]
[null,"镀锌地桩 ∠5×50×2500","根","38"]
[null,"名称：镀锌扁铁  5*50","米","27"]
["3.3.4","防火堵洞"]
[null,"防火涂料、堵洞、隔板及阻燃槽盒 防火涂料","KG","11.20"]
["3.3.5","生产工具、耗材","批","1"]
["3.3.6","营配信息系统工程资料","项","1"]
[3.4,"措施费","项",1]
[4,"调试工程量"]
[4.1,"电力变压器系统","项","1"]
[4.2,"接地系统","项","1"]
[4.3,"避雷器","项","1"]
[4.4,"电容器","项","1"]
[4.5,"措施费","项","1"]
[5,"勘察设计费","项","1"]